CESR Machine Studies Meeting 28 March 2002 JAC — SCMATING Knobs 1, 2, and 3 — Phase and Coupling Measurements

HEP conditions on 1s with single bunch e^+ of 6 mA

***********************************************
 Lattice = 1S_V2 type = STANDARD
 energy = 1S_ON sen1 = 1795.29 sen2 = 4946.70 dipole status = 1
 Set BIGGRP POSCSR ELCSR ELTOLUM POSTOP COLLIDE SCIR HEP CESR_RF
 Num 79929 79912 79957 78551 78294 79977 79954 79986 79673
 Orb 0 0 0 0 0 0 0 0 0
***********************************************
 POSLIN POSSYN ELLIN ELSYN
  80051 80052 79944 79945

SCMATING 1: −250 ⇒ +250 cu

SCMATING 1 works (as seen also on March 12 by DLR)

2 28 March 2002

SCMATING 2: 1000 ⇒ 500 cu

Small effect on coupling

3 28 March 2002

SCMATING 3: 1000 ⇒ 500 cu

Vertical tune moves ≃ 3 kHz during adjustment

Some action in north IP

4 28 March 2002